The information on archive.

The author of model and converting: Trall.

The full name: Mercedes-Benz ML 500.

The version: 1.0 (Stock)

Purpose: Model of the automobile for game Grand Theft Auto: San Andreas.

Quantity of ranges in model: 100457

Date of release: on September, 4, 2005.

Installation: manual, the instruction is see lower.

Model replaced in game: Landstalker.

Initial Internet - source: http://www.worldgamez.alfaspace.net/

And also we soon move here: http://www.worldgamez.ovl.ru/

Features of model. The small description.

Before you my best work at present. Absolutely all details are executed in 3d and with the maximal accuracy. I think about quality all this.:) In model all features and opportunities GTA are used: SA. If to speak more precisely that in model are available: 3 extras (look what;)), real light of lanterns, 2 functioning neon antifog headlights, illumination of numbers at night, an opportunity of tuning, including installation nitro, wheels and hydraulics, still more many pleasant and useful trifles. In general swing, establish and forward, to plough open spaces of state. ;)

Conditions of use.

Attention!!! During 30 days after release the model is exclusive for http://www.worldgamez.alfaspace.net/ On the expiration of this term archive can freely be distributed on the Internet. Please, adhere to these terms.

At the publication on the site it is necessary to write necessarily the author, a homepage and to place an applied screenshot.

At accommodation on the Internet it is forbidden to delete or change the files contained in archive. Addition of the additional text document or html-page is supposed.

It is forbidden to convert, modernize, use details and to use in commercial objectives without my sanction.

Simply write on E-mail or in ICQ and we shall agree upon all.

Please, respect my work!

The instruction on installation in game.

For installation you will need program IMGTool v2.0 With its help it is necessary to open a file gta3.img (GTA-SanAndreas\models). Then it is necessary to find and remove old files landstal.dff and landstal.txd (F2> landstal> Enter> Delete> Delete). Now we add new files landstal.dff and landstal.txd (Ctrl+A). In order to prevent mistakes to delete and add files it is necessary on one. When you have executed these actions, we close IMGTool.

Now it is necessary to make adjustments of the machine in three files (GTA-SanAndreas\data) which open by means of the standard program "Notebook". In each of these files it is necessary to replace a line which begins the name of model. Correct adjustments of the machine are below resulted.

handling.cfg

LANDSTAL 2100.0 6000.0 3.0 0.0 0.2 -0.30 75 0.60 0.80 0.51 5 235.0 27.7 15 4 P 10.0 0.53 1 32.0 1.50 0.13 0.0 0.18 -0.12 0.5 0.5 0.44 0.30 95000 00002020 00400004 1 2 0

vehicles.ide

400, landstal, landstal, car, LANDSTAL, LANDSTK, null, normal, 10, 0, 0, -1, 0.8, 0.8, 0

carcols.dat

landstal, 0,0, 4,4, 13,13, 25,25, 41,41, 43,43, 53,53, 119,119

carmods.dat

landstal, nto_b_l, nto_b_s, nto_b_tw

If all of you have correctly made, there will be no various bugs and the car will look as on a screenshot.

History M-klasse

It would seem, sale ML and without that on rise - is not present, time to be updated. First party M-Klasse have let out in 1997, since then worldwide has parted 620 thousand ML, mainly across America. It's time to go! Honour in Stuttgart know. The second generation though is not too beaten out from a stylistic outline habitual to us M-Klasse, but on technical power will give odds to many advanced off-road cars.
New ML almost on centimeter is lower than the predecessor, why it seems, that it keeps for a ground even more strong. Due to downturn of growth and design completions the factor of aerodynamic resistance has fallen with 0,39 up to 0,34 is at an off-road car! More "combed" back, with terrible lines on lateral panels and air inlets on a cowl, with new transparent optics ML reminds the rocket filled and ready to start. But the main thing - inside. On new M-Klasse the modified suspension brackets (it was possible to lower noise and vibration from wheels) and three new motors will appear. The most long-awaited - diesel V6 which will replace former 5-cylinder. ML 320CDI will please the owner with 224 horsepowers and 510 N*m the twisting moment already at 1600 rev/min. It designate for a role « itself off-road`s ». Who now will name ML citycar? Well unless only the convinced opponent of mark. For surcharge yours M-Klasse will improve special offroad`s a package: A lowering number in transmission, manual or automatic blocking of differentials (one - interaxal, another - on a back axis) and suspension bracket Airmatic specially modified under bad roads. This suspension bracket allows to change a road gleam within the limits of 110 mm. With such set maximal top M-Klasse passes for 290 mm. To it at all and 60-centimetric fords!

(On materials of magazine "За рулем ")

The information on me.

Trall aka Сергеев Саня(16.02.88) Russia, Krasnodar.
My E-mail: Trall@worldgamez.ovl.ru or Trall-Kuban-Krr@yandex.ru
MyICQ: 306-964-952
My site: http://www.worldgamez.alfaspace.net/

Gratitude.

Shock-For friendship and support.

Fl@sh - for friendship, support, advice after work and search of structures.

DMB-For the help on adjustments of model.

D4Ramm5-For friendship and the help on converting.

Pumbars-For support and the help on converting.

Forester-For the help on converting.

Viper-For advice and Zmodeler2.

Vint-For the help on converting.

And also I express huge gratitude to all team GTRMotorz and all forum GTA.COM.UA.

All THANKS!

On all arisen questions address on ICQ or E-mail. I shall be glad to answer.

Copyright © 2005 by Trall. All rights reserved. .:.:GTR Motorz:.:. ©